Link'd DMR CPS 1.0.0-rc.2 (win-x64)

1. Keep this entire folder together; do not move only the EXE.
2. Connect and unlock one CJ-1, then approve this computer if USB debugging asks.
3. Run LinkdDmr.Cps.exe.
4. Choose Radio > Connect to Link'd app on CJ-1, then read the RF codeplug.

The radio must have a Link'd app build with the CPS companion bridge.
CPS does not access owner recordings, archives, credentials, or privacy keys.
See RELEASE-NOTES.md and SIGNING-STATUS.txt before programming.
